

**Table of Contents**

[1. What is the LifeStyle HD? 1](#_Toc329089876)

[2. Safety Precautions 2](#_Toc329089877)

[3. Package 3](#_Toc329089878)

[4. Overview of LifeStyle HD 4](#_Toc329089879)

[**1) Front side 4**](#_Toc329089880)

[**2) Rear side 5**](#_Toc329089881)

[5. How to install 6](#_Toc329089882)

[**5.1 Connecting power cable 6**](#_Toc329089883)

[6. How to use Front Controller 7](#_Toc329089884)

[**6.1 Buttons on the front controller 7**](#_Toc329089885)

[**1) Front side 7**](#_Toc329089886)

[**2) Bottom and left side 8**](#_Toc329089887)

[7. Use the basic functions 9](#_Toc329089888)

[**1) Power on/off 9**](#_Toc329089889)

[**2) Adjusting the magnification 9**](#_Toc329089890)

[**3) Changing the color mode 10**](#_Toc329089891)

[**4) Adjusting contrast 11**](#_Toc329089892)

[**5) Using a PC with LifeStyle HD 11**](#_Toc329089893)

[**6) Using the Markers 12**](#_Toc329089894)

[8. Using the advanced feature 15](#_Toc329089895)

[**1) Selecting the various color modes 15**](#_Toc329089896)

[**2) Switching PICTURE/TEXT Mode 18**](#_Toc329089897)

[**3) Using the Focus Lock 18**](#_Toc329089898)

[**4) Adjusting the transparency of Window Marker 19**](#_Toc329089899)

[**5) Initialization 19**](#_Toc329089900)

[9. Using the Reading table 20](#_Toc329089901)

[**1) Moving the Reading table 20**](#_Toc329089902)

[**2) Lock/Unlock the Reading table 20**](#_Toc329089903)

[10. Light on/off 21](#_Toc329089904)

[11. Troubleshooting 22](#_Toc329089905)

[12. Technical Specifications of the LifeStyle HD 23](#_Toc329089908)

[13. Warranty 25](#_Toc329089909)

2. What is the LifeStyle HD?

Thanks for purchasing LifeStyle HD.

LifeStyle HD is an electronic magnifier for the low vision and the elderly to read books, manuals, grocery information with the large screen monitor.

**ZOOM**

You can change magnification level for your convenience depending on the size of text.

**COLOR**

LifeStyle HD provides you with the various color modes. You can select the color that best matches your needs.

**CONTRAST**


You can adjust the contrast to see the image clearly irrespective of the material being viewed.

1. Safety Precautions

Please read the following the safety precaution carefully before using the LifeStyle HD to protect both yourself and the LifeStyle HD

1. Do not use damaged power plug or unsuitable outlet to prevent electric shock or fire.
2. Do not touch power plug with wet hands to prevent electric shock.
3. Do not disassemble, remodeling or repair by unauthorized person. It may damage the unit and void the product warranty.
4. Install the unit in flat and stable place. Put on a table enough to bear the weight of your LifeStyle HD.
5. Do not pull down monitor too aggressively. It can cause LifeStyle HD to fall down.
6. Do not press down the reading table when moving table is pulled toward you. The unit may fall down.
7. Do not disconnect or connect any cable when the power is on. It may damage LifeStyle HD.
8. Do not use this unit in high humidity and/or high temperature such as over 40 Celsius degrees.
9. Package

The LifeStyle HD consists of the following items.





**LifeStyle HD**

**User manual**

**DVI-D Cable**

**Power cable**



1. Overview of LifeStyle HD

### **Front side**

**(1)**

**(2)**

**(3)**

**(6)**


**(5)**

**(4)**



1. LCD monitor
2. Front controller
3. Reading table locker
4. Reading table
5. Camera module
6. Monitor arm

### **Rear side**



**(8)**

**(7)**

1. DVI-D port
2. AC power port
3. How to install

## **5.1 Connecting power cable**

You can make the LifeStyle HD ready to be used simply by connecting the power cable to the AC power port. Connect the other end of the AC power cable to outlet.





1. How to use Front Controller

## **6.1 Buttons on the front controller**

The buttons are on the front, bottom and left sides of the front controller.

How to use those buttons will be explained on Chapter 7 of this user manual.

### **Front side**



1. **Color mode buttons**

Left: Previous color button

Right: Next color button

1. **Zoom in/out buttons**

Up (+): Zoom in button

Down (-): Zoom out button

1. **Power button**
2. **Power LED**

### **Bottom and left side**



1. **Switching PC/CCTV button**
2. **Marker button**
3. **Moving marker buttons**

Left: Left moving marker button

Right: Right moving marker button

1. **Contrast adjustment knob**
2. Use the basic functions

|  |
| --- |
| **※Before using LifeStyle HD**  In order to prevent tiredness of your eyes, you need to rest your eyes every 5, 10 or 15 minutes while using LifeStyle HD. Find out the best using time for you. After 30 minutes reading, please take a break to relieve your eyes. |

### **Power on/off**

To turn on the power of LifeStyle HD, press the **Power button**. The **Power button** is located on the far right of the front controller. Press the **Power button** one more time to turn the LifeStyle HD off while it’s on.

### **Adjusting the magnification**

You can adjust the magnification rate on the screen of LifeStyle HD. The LifeStyle HD can magnify from 2.7X to 84X. (19” Monitor)

#### ① Adjust the magnification rate

* To increase the magnification rate, press the **Zoom in** **button**.
* To decrease the magnification rate, press the **Zoom out** **button**.
* As you press and hold the buttons, the magnification rate is adjusted continuously while you are pressing it.

**(Note)** If you increase the magnification rate continuously by pressing **Zoom in** **button**, the magnification mode will be changed from optical zoom to digital zoom mode. At the digital zoom mode, magnification rate will be increased discretely, not continuously.

#### ② Find location function

* By using Find location function, you can find the point where you are reading on your document on the reading table.
* Press **Zoom in** **button** and **Zoom out** **button** simultaneously, then the magnification rate will be decreased at once and you can find where you are reading on the document.
* By releasing both **Zoom in** and **Zoom out** **buttons**, the magnification rate will return to the rate that you were using before pressing both buttons.

### **Changing the color mode**

You can change the color combinations of the text and background on the screen for the best matches of your needs.

The LifeStyle HD provides 7 color modes.

1. Natural Color

2. White text on Black background

3. Black text on White background

4. Gray

5. Yellow text on Black background

6. Yellow text on Blue background

7. Green text on Black background

Press the **Previous color button** to change to the previous color mode. To change to the next color mode, press the **Next color button**.

### **Adjusting contrast**



According to the paper types and colors of letters and backgrounds of documents or books that you are reading, you need to adjust the contrast so that you can read the documents or books clearly. You can adjust contrast by using the Contrast adjustment knob at the far-right-bottom side of Front controller.

* Move the **Contrast adjustment knob** to the left to decrease the contrast value.
* Move the **Contrast adjustment knob** to the right to increase the contrast value.

### **Using a PC with LifeStyle HD**

The **Switching PC/CCTV button** is located at the left side of front controller. To use this button, connect a PC to the LifeStyle HD in advance.

#### ① Connecting a PC

To connect a PC with the LifeStyle HD, follow these steps below:

1. Turn the LifeStyle HD and the PC off.
2. DVI-D input port is located at rear side of the LifeStyle HD. Connect one end of DVI-D cable to the PC and other end to the DVI-D input port of LifeStyle HD.
3. Power on the PC. The image of PC will be displayed on the monitor screen of LifeStyle HD.
4. Afterwards, power on the LifeStyle HD. The image of LifeStyle HD will be displayed on the screen.

#### ② Switching the PC/CCTV

After connecting a PC with LifeStyle HD, you can switch between the screen of PC and CCTV.

1. In CCTV screen, press the **Switching PC/CCTV button**. It changes to the screen of PC.
2. In PC screen, press the Switching PC/CCTV button again, it changes to the screen of LifeStyle HD.

**(Note)** When you press the Switching PC/CCTV button while the PC is off, [**NO SIGNAL**] will be displayed on the screen. When [**NO SIGNAL**] shows up while the PC is on, reboot the PC.

### **Using the Markers**

The Marker helps you to focus on the part that you are reading by narrowing the display area of window markers or by underling under the sentence that you are reading. In that way, it can improve your reading ability.

To execute the marker, press the **Marker** **button** which is located at the far-left-bottom side of the front controller.

#### ① Changing the Marker type

Pressing the **Marker** **button**, the Horizontal Line Maker will be displayed on the screen.

There are 4 kinds of markers.

|  |  |
| --- | --- |
| * Horizontal Line Marker   ABCDEFGHIJKLMNOPQR  ABCDEFGHIJKLMNOPQR  ABCDEFGHIJKLMNOPQR  ABCDEFGHIJKLMNOPQR | * Vertical Line Marker   ABCDEFGHIJKLMNOPQR  ABCDEFGHIJKLMNOPQR  ABCDEFGHIJKLMNOPQR  ABCDEFGHIJKLMNOPQR |
| * Horizontal Window Marker   ABCDEFGHIJKLMNOPQR  ABCDEFGHIJKLMNOPQR  ABCDEFGHIJKLMNOPQR  ABCDEFGHIJKLMNOPQR | * Vertical Window Marker   ABCDEFGHIJKLMNOPQR  ABCDEFGHIJKLMNOPQR  ABCDEFGHIJKLMNOPQR  ABCDEFGHIJKLMNOPQR |

To cancel the marker option, press the Marker button again at the Vertical Window Marker mode.

#### ② Adjusting the location/width of Marker

You can adjust the location of line marker in Line marker modes. Or you can adjust the width of window marker in Window marker modes.

To adjust the location/width of markers, press the **Moving marker buttons**. **Moving marker** **buttons** are located right next to the Marker button. The left button is the **Left moving marker** **button**. The right button is the **Right moving marker** **button**.

How to adjust the Location/range as marker type is different.

* When the Line Marker mode is activated
* **Horizontal Line Marker:**

Pressing the **Left moving marker** **button** moves it up.

ABCDEFGHIJKLMNOPQR

ABCDEFGHIJKLMNOPQR

ABCDEFGHIJKLMNOPQR

ABCDEFGHIJKLMNOPQR

Pressing the **Right moving marker** **button** moves it down.

* **Vertical Line Marker:**

Pressing the **Left moving marker** **button** moves it to the left.

ABCDEFGHIJKLMNOPQR

ABCDEFGHIJKLMNOPQR

ABCDEFGHIJKLMNOPQR

ABCDEFGHIJKLMNOPQR

Pressing the **Right moving marker** **button** moves it to the right.

* When the Window Marker mode is activated
* **Horizontal/Vertical Window Marker:**

Pressing the **Left moving marker** **button**, the window gets wider.

Pressing the **Right moving marker** **button**, the window gets narrower.

ABCDEFGHIJKLMNOPQR

ABCDEFGHIJKLMNOPQR

ABCDEFGHIJKLMNOPQR

ABCDEFGHIJKLMNOPQR

ABCDEFGHIJKLMNOPQR

ABCDEFGHIJKLMNOPQR

ABCDEFGHIJKLMNOPQR

ABCDEFGHIJKLMNOPQR

1. Using the advanced feature

### **Selecting the various color modes**

The LifeStyle HD provides 7 color modes. The color modes 1 to 3 are unchangeable but 4 to 7 are selectable.

1. Natural Color

2. White text on Black background

3. Black text on White background

4. Gray: **Selectable**

5. Yellow text on Black background : **Selectable**

6. Yellow text on Blue background : **Selectable**

7. Green text on Black background : **Selectable**

#### ① Changing the color mode

To change the color mode, please follow the steps below;

1. Choose any mode among color modes 4, 5, 6 or 7 above which you want to change the color by using the **Color mode** **buttons**.
2. Once you select the color mode, press both the **Previous color** and **Next color** **buttons** for more than 2 seconds.
3. [**MODE SETUP**] will show up and then [**SELECT COLOR**] will be displayed on the screen.
4. Move to the color mode that you want to change by pressing either the **Previous color** or **Next color** **buttons**. (Refer to the Color table)
5. Press both the **Previous** and **Next color buttons** at once. [**SAVE? YES**] will be displayed on the screen.
6. If you want to save the color combination you have chosen, press both the **Previous** and **Next color buttons** at once one more time. [**CONFIRM**] will be displayed on the screen and it is saved.
7. If you don’t want to save, press the **Previous** or **Next color buttons**. [**SAVE? NO**] will be displayed on the screen.
8. Pressing both the **Previous** and **Next color buttons**, [**EXIT**] will be displayed on the screen and it is canceled.

#### ② Color table

The color of the text and background is displayed on the screen after executing the [**MODE SETUP**].

The following description is how to check the color table.

* When you execute the [**MODE SETUP**] in the Yellow text on Black background;
* If you press the **Next color button**, the Red text on White background will be displayed on the screen.
* If you press the **Previous color button**, the Black text on Yellow background will be displayed on the screen.
* When you execute the [**MODE SETUP**] in the Green text on Black background;
* If you press the **Next color button**, the Cyan text on black background will be displayed on the screen.
* If you press the **Previous color button**, the Black text on Green background will be displayed on the screen.

|  |  |
| --- | --- |
| **Text** | **Background** |
| GRAY | |
| BLACK | RED |
| RED | BLACK |
| BLACK | GREEN |
| GREEN | BLACK |
| CYAN | BLACK |
| BLACK | CYAN |
| BLACK | MAGENTA |
| MAGENTA | BLACK |
| BLACK | YELLOW |
| YELLOW | BLACK |
| RED | WHITE |
| WHITE | RED |
| GREEN | WHITE |
| WHITE | GREEN |
| BLUE | WHITE |
| WHITE | BLUE |
| WHITE | CYAN |
| CYAN | WHITE |
| BLUE | YELLOW |
| YELLOW | BLUE |
| MAGENTA | WHITE |
| WHITE | MAGENTA |
| GREEN | RED |
| RED | GREEN |
| BLUE | RED |
| RED | BLUE |
| YELLOW | RED |
| RED | YELLOW |

### **Switching PICTURE/TEXT Mode**

The LifeStyle HD allows you to alternate between PICTURE and TEXT Mode.

The default value is PICTURE Mode. The PICTURE Mode is very convenient for users to see the photos or pictures on the books.

The TEXT Mode is convenient for reading letters as the gaps between characters are wide.

To switch the TEXT Mode, follow these steps below:

1. Press the **Switching PC/CCTV button** for more than 2 seconds.
2. It changes to TEXT mode.
3. In TEXT Mode, pressing the **Switching PC/CCTV button** for more than 2 seconds again, it changes to PICTURE mode.

### **Using the Focus Lock**

The LifeStyle HD provides automatic focus. Not to make the LifeStyle HD focus on your hand or the pen instead of the letters when you are writing, use the Focus lock.

1. Press both the **Left and the Right moving marker button** for more than 2 seconds.
2. [**FOCUS LOCK**] will be displayed on the screen.
3. To cancel the Focus lock, press both the **Left and the Right moving marker button** at once again.
4. [**FOCUS AUTO**] will be displayed on the screen.

Also, when you reboot the LifeStyle HD, it returns to the Automatic focus.

### **Adjusting the transparency of Window Marker**

In window marker mode, you can adjust the transparency.

To adjust the transparency of window marker, follow these steps below:

1. In window marker mode, press the **Marker button** for more 2 seconds.
2. [**WINDOW OPACITY 100**] will be displayed on the screen.
3. Press the **Left moving marker button** to decrease the value. Press the **Right moving marker button** to increase the value.
4. Once you select the value of transparency, press the **Marker button**.
5. [**SAVE? YES**] will be displayed on the screen.
6. If you want to save the value you prefer, press the **Marker button**. [**CONFIRM**] will be displayed and it is saved.
7. If you don’t want to save, press the **Left or Right moving marker button**. [**SAVE? NO**] will be displayed on the screen.
8. Press the **Marker button**. [**EXIT**] will be displayed and it is canceled.

### **Initialization**

You can initialize the LifeStyle HD owing to the user’s fault or malfunction.

1. Turn the LifeStyle HD on by pressing the **Power button** while pressing the **Switching PC/CCTV button**.
2. Release the **Switching PC/CCTV button** when [**INITIALIZATION**] shows up with a beep sound. The LifeStyle HD will reboot and return to factory defaults.
3. Turn the LifeStyle HD off and turn it back on, the initialization will be completed.
4. Using the Reading table

When you want to magnify the object that does not display on the screen at once, use the Reading table.

### **Moving the Reading table**

The Reading table moves to the left-right and up-down when you hold the handles of the Reading table.



### **Lock/Unlock the Reading table**

The **Reading table locker** at the front of the Reading table allows you to fix the Reading table. To lock the Reading table, move the **Reading table locker** all the way to the right. To unlock the Reading table, move the **Reading table locker** to the left.



1. Light on/off

When you turn on the LifeStyle HD, the light is on. Turn off the light, when you view the reflexible objects or the light is too light.

The **Light switch** is under the Camera module.



1. Troubleshooting

### **The image on the screen is not clear**

* In Focus Lock mode, it doesn’t focus automatically. Switch to the Focus Auto by pressing the **Switching PC/CCTV button**.
* Adjust the contrast by using the **Contrast adjustment knob**.

### **Cannot execute the mode setup in color mode**

* Check the current color mode. Only in mode 4 to 7, you can select the different color mode.
* Check the Marker. You cannot execute the mode setup while using the Marker.

1. Technical Specifications of the LifeStyle HD

|  |  |
| --- | --- |
| **Model** | HD730 |
| **Magnification** | 2.7X ~ 84X (19” monitor)  3.1X ~ 95X (22” monitor)  3.4X ~ 105X (24” monitor) |
| **Power** | 100~240V~, 50/60Hz. 2A, 65W |
| **Size** | 19” monitor: 48cm(H) x 44cm(W) x 51cm(D)  22” monitor: 52cm(H) x 52cm(W) x 52cm(D)  24” monitor: 54cm(H) x 57cm(W) x 53cm(D) |
| **Basic Color Mode** | 1. Natural Color  2. White text on Black background  3. Black text on White background  4. Gray\_**Selectable**  5. Yellow text on Black background\_**Selectable**  6. Yellow text on Blue background\_**Selectable**  7. Green text on Black background\_**Selectable** |
| **Select Color in Mode Setup** | - 15 kinds of select color in Mode Setup  Gray, Black/Red, Black/Green, Black/Cyan, Black/Magenta, Black/Yellow, Red/White, Green/White, Blue/White, Cyan/White, Magenta/White, Blue/Yellow, Green/Red, Blue/Red, Yellow/Red  - Support Negative Mode for each color mode except Gray |
| **Weight** | 16.5 Kg (19” monitor)  17.2 Kg (22” monitor)  18.0 Kg (24” monitor) |
| **Output Resolution** | High Definition(HD) |

(**NOTE**) This user manual will be differed from actual operation due to improved function of products and it is subject to change and modified without prior notice.

1. Warranty
2. Warranty term is 2 years from your purchasing.
3. Warranty does not cover the problem due to the user’s fault.

(**Note**) The warranty term will be different from each country.

****

NOTE: This equipment has been tested and found to comply with the limits for a Class B digital device, pursuant to part 15 of the FCC Rules. These limits are designed to provide reasonable protection against harmful interference in a residential installation.

This equipment generates, uses and can radiate radio frequency energy and, if not installed and used in accordance with the instructions, may cause harmful interference to radio communications. However, there is no guarantee that interference will not occur in a particular installation. If this equipment does cause harmful interference to radio or television reception, which can be determined by turning the equipment off and on, the user is encouraged to try to correct the interference by one or more of the following measures:

- Reorient or relocate the receiving antenna.

- Increase the separation between the equipment and receiver.

- Connect the equipment into an outlet on a circuit different from that to which the receiver is connected.

- Consult the dealer or an experienced radio/TV technician for help.

CAUTION: Changes or modifications not expressly approved by the manufacturer responsible for compliance could void the user’s authority to operate the equipment.